${header_size} 1001
${originator_name}; Brem, Benjamin; Gysel-Beer,  Martin
${lab}, Paul Scherrer Institute, PSI,,,, 5232, Villigen PSI, Switzerland
${submitter_name}
GAW-WDCA EMEP CREATE ACTRIS
1 1
${start_day}     ${rev_day}
${dt}
Days from the file reference point (start_time)
${nvars}
${scale_factors}
${vars_fill}
end_time of measurement, days from the file reference point
${vars_long_name}
0
${nlines_aux_com}
Data definition:                EBAS_1.1
Set type code:                  ${set_type_code}
Station code:                   ${station}
Platform code:                  ${platform}
Timezone:                       UTC
Startdate:                      ${start_time}
Timeref:                        00_00
Revision date:                  ${prod_time}
Component:                      ${component}
Unit:                           ${unit}
Matrix:                         ${matrix}
Period code:                    ${period_tag}
Resolution code:                ${dt_tag}
Sample duration:                ${dt_tag}
Laboratory code:                ${lab}
Instrument type:                ${instrument}
Instrument manufacturer:        ${brand}
Instrument model:               ${model}
Instrument name:                ${instr_name}
Instrument serial number:       ${sn}
Method ref:                     ${method_ref}
Orig. time res.:                ${dt_raw_tag}
File name:                      ${fname}
Station WDCA-ID:                ${wdca_id}
Station name:                   ${site}
Station GAW-Name:               ${site}
Station GAW-ID:                 ${gaw_id}
Measurement latitude:           ${latitude}
Measurement longitude:          ${longitude}
Measurement altitude:           ${altitude}m
Station land use:               ${wmo_land_use}
Station setting:                ${wmo_setting}
Station GAW type:               ${gaw_type}
Station WMO region:             ${wmo_region}
Originator:                     ${originator}
Originator:                     Brem, Benjamin, benjamin.brem@psi.ch, Paul Scherrer Institute, PSI, Laboratory of Atmospheric Chemistry,,, 5232, Villigen PSI, Switzerland
Originator:                     Gysel-Beer, Martin, martin.gysel@psi.ch, Paul Scherrer Institute, PSI, Laboratory of Atmospheric Chemistry,,, 5232, Villigen PSI, Switzerland
Submitter:                     	${submitter}
Data level:                     ${lvl}
Version:                        1
Version description:            initial revision
Measurement height:             2m
Inlet type:                     Hat or hood
Inlet description:              Heated total aerosol inlet (25 degC), collects aerosols and hydrometeors smaller than 40 micrometers
Humidity/temperature control:   Temperature conditioning at 25 deg. C
Humidity/temperature control description: Sample dried to below 20% RH due to the heated inlet
Volume std. temperature:        ${std_temp}K
Volume std. pressure:           ${std_pres}hPa
Measurement uncertainty:        0.2 ug/m3
Measurement uncertainty expl.:  includes statistical uncertainty of individual sample and calibration uncertainty
Zero/negative values code:      Zero/negative possible
Zero/negative values:           Zero and neg. values may appear due to statistical variations at very low concentrations
Standard method:                None
Comment:                        The data has been processed in Tofware and R. A constant CE of 1 has been applied. Acquisition temperature = 298.15 K, acquisition pressure = 650 hPa, STP correction applied with these fixed values.  
Acknowledgement:                For using this data for any kind of publications, you must contact the data originator(s), in terms of acknowledgment
start_time     end_time       ${vars_tag}
