BMW_startup.xml Here some external parameters used in conjunction with the BMWlibs are set. There are different sections: * Common parameters which are used for any kind of function * Parameters for low energy uSR data analysis with given B(z) * Parameters for bulk uSR data analysis (currently only four model to calculate field distributions for a triangular vortex lattice) * Parameters for dynamical LF relaxation functions within the BMWlibs (mainly useful for testing purposes)

Common parameters: - debug : set it to 1 in order to obtain some information what is read from the xml-file - wisdom : sets the path to an FFTW-wisdom file - if there is no valid wisdom at the given path, wisdom handling will be disabled - wisdom_float : sets the path to a float-FFTW-wisdom file - if there is no valid wisdom at the given path, wisdom handling will be disabled (at the moment only used for LF-relaxation functions) - delta_t : time resolution of P(t) in microseconds - delta_B : field resolution of P(B) in Gauss

LF-relaxation parameters: - delta_t_LF : time resolution of P(t) in microseconds for the Laplace transforms involved in the dynamical LF-relaxation calculations - N_LF : length of the Laplace transforms involved in the dynamical LF-relaxation calculations

LEM parameters (if the LEM tag is present it is expected that the data_path tag contains a valid path): - data_path, energy_list : Defines path/prefix, energy-labels and energies (keV) of TrimSP-rge-files The expected file-names are then: data_path + energy_label + .rge - N_theory : determines the number of points in "real space" where the theory function B(z) will be calculated (if necessary)

bulk parameters: - N_VortexGrid : determines the number of points used for the calculation of the vortex lattice field distribution (the grid will be N*N)
0
none
none
0.01
0.5
512
0.00004
524288
profiles/TestProfile-
5000
02_0
2.0
05_0
5.0
07_5
7.5
10_0
10.0
12_0
12.0
16_0
16.0
18_0
18.0
20_0
20.0
22_0
22.0
24_0
24.0