Next: Detector files Up: The detector description Previous: The detector description

## Experimental setting
Keywords: LEMuSR_Simulation

After passing trigger detector, the muons beam is focused through electrostatic lenses either to the sample or a micro channel detector. The simulation allows this flexibility and one can change from the cryostat to mcp, and tune the voltages at will. The commands will be described later (2.2).