{
    "menuFlags":{
        "hasFile": 1,
        "loadInitFile": 1,
        "hasDaq":  1,
        "hasH5" : 1,
	"hasEpics" : 1
    },
   "ElogBooks": {
        "SLS+Development": {
            "url": "https://elog-gfa.psi.ch:443/SLS+Development",
            "destination": "/afs/psi.ch/intranet/Controls/tmp/elog/ePic/sls/"
        },
        "SLS+Measurement+Data": {
            "url": "https://elog-gfa.psi.ch:443/SLS+Measurement+Data",
            "destination": "/afs/psi.ch/intranet/Controls/tmp/elog/ePic/sls/"
        }
    },
    "Elog":{
        "useELOGenv": 0,
        "host": "elog-gfa.psi.ch",
	"book": "SLS+Development",
	"url": "https://elog-gfa.psi.ch/SLS+Development",
	"destination": "/afs/psi.ch/intranet/Controls/tmp/bdbase/ePic/",
	"category": ["Info","Measurement"],
	"system"  : ["","Beamdynamics","Controls", "Diagnostics", "Electric supply", "Insertion-devices", "Laser", 
		     "Magnet Power Supplies", "Operation", "RF", "Safety", "Vacuum", "Water cooling", "Other", "Unknown"],
	"domain"  : ["","Injector","Linac1","Linac2","Linac3","Aramis","Aramis Beamlines","Athos","Athos Beamlines"],
	"section" : [ [""],
		      [""]
		      ]
    },
    "stdlog":{
        "destination": "/tmp/"
    },  
    "screenshot": {
        "destination": "/tmp/"
    },
    "url": {
        "archiver"  : "https://ui-data-api.psi.ch/prepare?channel=sf-archiverappliance/",
	"databuffer": "https://ui-data-api.psi.ch/prepare?channel=sf-databuffer/"
    },
    "OpMsg":{
        "pvDate1" :"ACOAU-ACCU:OP-DATE1",
        "pvMsg1"  :"ACOAU-ACCU:OP-MSG1",
	"upTime"  : "ACOAU-ACCU:UT-HOURS"
    }, 
    "PCT":{
        "current": "ARIDI-PCT:CURRENT",
	"curROC": "ARIDI-PCT:CUR-ROC",
	"tauHour": "ARIDI-PCT:TAU-HOUR",
	"injRate": "ARIDI-PCT:INJ-RATE"
    },
    "OFB":{
        "xrms": "ARIDI-BPM:OFB-XRMS",
	"yrms": "ARIDI-BPM:OFB-YRMS",
	"xmean": "ARIDI-BPM:OFB-XMEAN",
	"ymean": "ARIDI-BPM:OFB-YMEAN"
    },
    "hdfGroups": {
        "General":["Created","Author","Application","Comment","Filepath","Process","UID","User"]
    },
    "h5Machine": {
        "charge":   "SINEG01-DICT215:B1_CHARGE_AVERAGE-OP",
        "laser":    "SLG-LGEN:WHICH_LASER",
        "repRate":  "SIN-TIMAST-TMA:Beam-Appl-Freq-RB",
        "beamDest": "SF:MODE_AR",
        "energy":   "SF:ENERGY_AR"
    },
    "h5Data": {
        "dataSet": ["timestamp","data", "pulse_id", "timestamp_offset"]  
    }
}
