Commands to configure the receiver 