#*************************************************************************
# Copyright (c) 2002 The University of Chicago, as Operator of Argonne
#     National Laboratory.
# Copyright (c) 2002 The Regents of the University of California, as
#     Operator of Los Alamos National Laboratory.
# EPICS BASE is distributed subject to a Software License Agreement found
# in file LICENSE that is included with this distribution.
#*************************************************************************

=title Event Record (event)

The normal use for this record type is to post an event and/or process a
forward link. Device support for this record can provide a hardware interrupt
handler routine for I/O Event-scanned records.

=head2 Parameter Fields

The records in this field fall into the following groups of parameters:

=over

=item *

scan parameters

=item *

read parameters

=item *

event number parameters

=item *

simulation mode parameters

=back

=recordtype event

=cut

recordtype(event) {
	include "dbCommon.dbd"

=head3 Scan Parameters

The event record has the standard fields for specifying under what circumstances
it will be processed. If the SCAN field specifies C<I/O Intr>, then device
support will provide an interrupt handler, posting an event number when an I/O
interrupt occurs. These fields are listed in L<Scan Fields>. In addition,
L<Scanning Specification> explains how the scanning fields work. Note that I/O
event scanning is only supported for those card types that interrupt.

=head3 Event Number Parameters

The VAL field contains the event number read by the device support routines. It
is this number which is posted. For records that use C<Soft Channel> device
support, it can be configured before run-time or set via dbPuts.

=fields VAL

=cut

	field(VAL,DBF_STRING) {
		prompt("Event Name To Post")
		promptgroup("40 - Input")
		special(SPC_MOD)
		asl(ASL0)
		size(40)
	}
	%#include "dbScan.h"
	field(EPVT, DBF_NOACCESS) {
		prompt("Event private")
		special(SPC_NOMOD)
		interest(4)
		extra("EVENTPVT epvt")
	}

=head3 Input Specification

The device support routines use the address in this record to obtain input. For
records that provide an interrupt handler, the INP field should specify the
address of the I/O card, and the DTYP field should specify a valid device
support module. Be aware that the address format differs according to the card
type  used. See L<Address Specification> for information on the format of
hardware addresses and specifying links.

For soft records, the INP field can be a constant, a database link, or a channel
access link. For soft records, the DTYP field should specify C<Soft Channel>.

=fields INP, DTYP

=cut

	field(INP,DBF_INLINK) {
		prompt("Input Specification")
		promptgroup("40 - Input")
		interest(1)
	}

=head3 Operator Display Parameters

See L<Fields Common to All Record Types> for more on the record name (NAME) and
description (DESC) fields.

=fields NAME, DESC

=head3 Alarm Parameters

The Event record has the alarm parameters common to all record types. L<Alarm
Fields> lists other fields related to alarms that are common to all record
types.

=head3 Simulation Mode Parameters

The following fields are used to operate the event record in the simulation
mode.  See L<Fields Common to Many Record Types> for more information on these
fields.

=fields SIOL, SVAL, SIML, SIMM, SIMS

=cut

	field(SIOL,DBF_INLINK) {
		prompt("Sim Input Specifctn")
		promptgroup("90 - Simulate")
		interest(1)
	}
	field(SVAL,DBF_STRING) {
		prompt("Simulation Value")
		size(40)
	}
	field(SIML,DBF_INLINK) {
		prompt("Sim Mode Location")
		promptgroup("90 - Simulate")
		interest(1)
	}
	field(SIMM,DBF_MENU) {
		prompt("Simulation Mode")
		interest(1)
		menu(menuYesNo)
	}
	field(SIMS,DBF_MENU) {
		prompt("Sim mode Alarm Svrty")
		promptgroup("90 - Simulate")
		interest(2)
		menu(menuAlarmSevr)
	}

=head2 Record Support

=head3 Record Support Routines

=head4 init_record

This routine initializes SIMM with the value of SIML if SIML type is a CONSTANT
link or creates a channel access link if SIML type is PV_LINK. SVAL is likewise
initialized if SIOL is CONSTANT or PV_LINK.

If device support includes C<init_record()>, it is called.

=head4 process

See next section.

=head3 Record Processing

Routine process implements the following algorithm:

=over

=item 1.

readValue is called. See L<Input Records> for more information.

=item 2.

If PACT has been changed to TRUE, the device support read routine has started
but has not completed reading a new input value. In this case, the processing
routine merely returns, leaving PACT TRUE.

=item 3.

If VAL E<gt> 0, post event number VAL.

=item 4.

Check to see if monitors should be invoked. Alarm monitors are invoked if the
alarm status or severity has chanet to 0.

=item 5.

Scan forward link if necessary, set PACT FALSE, and return.

=back

=head2 Device Support

=head3 Fields of Interest To Device Support

Each record must have an associated set of device support routines. The device
support routines are primarily interested in the following fields:

=fields PACT, DPVT, UDF, NSEV, NSTA, INP, PRIO

=head3 Device Support Routines

Device support consists of the following routines:

=head4 long report(int level)

This optional routine is called by the IOC command C<dbior> and is passed the
report level that was requested by the user.
It should print a report on the state of the device support to stdout.
The C<level> parameter may be used to output increasingly more detailed
information at higher levels, or to select different types of information with
different levels.
Level zero should print no more than a small summary.

=head4 long init(int after)

This optional routine is called twice at IOC initialization time.
The first call happens before any of the C<init_record()> calls are made, with
the integer parameter C<after> set to 0.
The second call happens after all of the C<init_record()> calls have been made,
with C<after> set to 1.

=head4 init_record

  init_record(precord)

This routine is optional. If provided, it is called by the record support
C<init_record()> routine.

=head4 get_ioint_info

  get_ioint_info(int cmd, struct dbCommon *precord, IOSCANPVT *ppvt)

This routine is called by the ioEventScan system each time the record is added
or deleted from an I/O event scan list. cmd has the value (0,1) if the record is
being (added to, deleted from) an I/O event list. It must be provided for any
device type that can use the ioEvent scanner.

=head4 read_event

  read_event(precord)

This routine returns the following values:

=over

=item *

0: Success.

=item *

Other: Error.

=back

=head3 Device Support For Soft Records

The C<Soft Channel> device support module is available. The INP link type must
be either CONSTANT, DB_LINK, or CA_LINK.

If the INP link type is CONSTANT, then the constant value is stored into VAL by
C<init_record()>, and UDF is set to FALSE. If the INP link type is PV_LINK, then
dbCaAddInlink is called by C<init_record()>.

C<read_event> calls recGblGetLinkValue to read the current value of VAL. See
L<Input Records> for details on soft input.

=cut

}
