#*************************************************************************
# Copyright (c) 2010 UChicago Argonne LLC, as Operator of Argonne
#     National Laboratory.
# Copyright (c) 2002 The Regents of the University of California, as
#     Operator of Los Alamos National Laboratory.
# EPICS BASE is distributed subject to a Software License Agreement found
# in file LICENSE that is included with this distribution. 
#*************************************************************************
#	Author:	Andrew Johnson
#	Date:	1 May 1995
#
#	Experimental Physics and Industrial Control System (EPICS)
#
#	CONFIG_SITE_ENV - EPICS Environment Parameter Site configuration file
#
# This file is read by the script base/src/libCom/env/bldEnvData.pl
# Variable definitions must take the form
#	VAR = VALUE
# or
#	VAR = "Value containing spaces"
# with each one on its own line.
# Enclosing spaces and "" will be trimmed.
#

#  Site-specific environment settings

## Time service:
# EPICS_TZ
#       Local timezone rules for vxWorks and RTEMS. The value follows the Posix
#       TZ environment variable's Mm.n.d/h format (see the IBM link below for
#       details). If TZ hasn't already been set when the osdTime timeRegister()
#       C++ static constructor runs, this parameter will be copied into the TZ
#       environment variable. Once the OS clock has been synchronized to NTP the
#       routine tz2timezone() will be run to convert TZ into the TIMEZONE
#       variable format that VxWorks needs.
#               https://developer.ibm.com/articles/au-aix-posix/

# Japan Standard Time, no DST:
#EPICS_TZ = "JST-9"

# Central European (Summer) Time:
#EPICS_TZ = "CET-1CEST,M3.5.0/2,M10.5.0/3"

# Greenwich Mean/British Summer Time:
#EPICS_TZ = "GMT0BST,M3.5.0/1,M10.5.0/2"

# US Eastern Standard/Daylight Time:
#EPICS_TZ = "EST5EDT,M3.2.0/2,M11.1.0/2"

# US Central Standard/Daylight Time:
EPICS_TZ = "CST6CDT,M3.2.0/2,M11.1.0/2"

# US Mountain Standard/Daylight Time:
#EPICS_TZ = "MST7MDT,M3.2.0/2,M11.1.0/2"

# US Pacific Standard/Daylight Time:
#EPICS_TZ = "PST8PDT,M3.2.0/2,M11.1.0/2"

# US Hawaiian Standard Time, no DST:
#EPICS_TZ = "HST10"


# EPICS_TS_NTP_INET
#	NTP time server ip address for VxWorks and RTEMS.
#	IOC will use its boot host if this is not set.
EPICS_TS_NTP_INET=

# IOC Shell:
# IOCSH_PS1
#	Prompt string
# IOCSH_HISTSIZE
#	Number of lines of command history to keep.
IOCSH_PS1="epics> "
IOCSH_HISTSIZE=50

# Log Server:
# EPICS_IOC_LOG_INET 
#	Log server ip addr.
# EPICS_IOC_LOG_FILE_NAME 
#	pathname to the log file.
# EPICS_IOC_LOG_FILE_LIMIT 
#	maximum log file size.
# EPICS_IOC_LOG_FILE_COMMAND 
#	A shell command string used to obtain a new 
#       path name in response to SIGHUP - the new path name will
#       replace any path name supplied in EPICS_IOC_LOG_FILE_NAME

EPICS_IOC_LOG_INET=
EPICS_IOC_LOG_FILE_NAME=
EPICS_IOC_LOG_FILE_COMMAND=
EPICS_IOC_LOG_FILE_LIMIT=1000000

