The CPU030 may need to have the nivxi path set correctly:
	From the vxWorks shell type vxitedit
	take option 2
	take option 3
	type list
	type modify 0
		type in the correct path when promped
		(the path should end in nivxi 
		and should traverse the niCpu030
		directories shipped with the 030
	type save
	type exit
	.
	.
	.


You may may need to setup front panel to backplane trigger
routing:

To take a TTL input and map it to VXI backplane ECL trigger 0
type in (to the vxWorks shell):

epvxiRouteTriggerECL(<logical address>, 1, 0)

where <logical address> specifies the card with the 
front panel trigger connection.

