#*************************************************************************
# Copyright (c) 2002 The University of Chicago, as Operator of Argonne
#     National Laboratory.
# Copyright (c) 2002 The Regents of the University of California, as
#     Operator of Los Alamos National Laboratory.
# EPICS BASE is distributed subject to a Software License Agreement found
# in file LICENSE that is included with this distribution.
#*************************************************************************
menu(selSELM) {
	choice(selSELM_Specified,"Specified")
	choice(selSELM_High_Signal,"High Signal")
	choice(selSELM_Low_Signal,"Low Signal")
	choice(selSELM_Median_Signal,"Median Signal")
}
recordtype(sel) {
	include "dbCommon.dbd" 
	field(VAL,DBF_DOUBLE) {
		prompt("Result")
		promptgroup("40 - Input")
		asl(ASL0)
		special(SPC_NOMOD)
	}
	field(SELM,DBF_MENU) {
		prompt("Select Mechanism")
		promptgroup("30 - Action")
		menu(selSELM)
	}
	field(SELN,DBF_USHORT) {
		prompt("Index value")
	}
	field(PREC,DBF_SHORT) {
		prompt("Display Precision")
		promptgroup("80 - Display")
		interest(1)
	}
	field(NVL,DBF_INLINK) {
		prompt("Index Value Location")
		promptgroup("30 - Action")
		interest(1)
	}
	field(INPA,DBF_INLINK) {
		prompt("Input A")
		promptgroup("41 - Input A-F")
		interest(1)
	}
	field(INPB,DBF_INLINK) {
		prompt("Input B")
		promptgroup("41 - Input A-F")
		interest(1)
	}
	field(INPC,DBF_INLINK) {
		prompt("Input C")
		promptgroup("41 - Input A-F")
		interest(1)
	}
	field(INPD,DBF_INLINK) {
		prompt("Input D")
		promptgroup("41 - Input A-F")
		interest(1)
	}
	field(INPE,DBF_INLINK) {
		prompt("Input E")
		promptgroup("41 - Input A-F")
		interest(1)
	}
	field(INPF,DBF_INLINK) {
		prompt("Input F")
		promptgroup("41 - Input A-F")
		interest(1)
	}
	field(INPG,DBF_INLINK) {
		prompt("Input G")
		promptgroup("42 - Input G-L")
		interest(1)
	}
	field(INPH,DBF_INLINK) {
		prompt("Input H")
		promptgroup("42 - Input G-L")
		interest(1)
	}
	field(INPI,DBF_INLINK) {
		prompt("Input I")
		promptgroup("42 - Input G-L")
		interest(1)
	}
	field(INPJ,DBF_INLINK) {
		prompt("Input J")
		promptgroup("42 - Input G-L")
		interest(1)
	}
	field(INPK,DBF_INLINK) {
		prompt("Input K")
		promptgroup("42 - Input G-L")
		interest(1)
	}
	field(INPL,DBF_INLINK) {
		prompt("Input L")
		promptgroup("42 - Input G-L")
		interest(1)
	}
	field(EGU,DBF_STRING) {
		prompt("Engineering Units")
		promptgroup("80 - Display")
		interest(1)
		size(16)
		prop(YES)
	}
	field(HOPR,DBF_DOUBLE) {
		prompt("High Operating Rng")
		promptgroup("80 - Display")
		interest(1)
		prop(YES)
	}
	field(LOPR,DBF_DOUBLE) {
		prompt("Low Operating Range")
		promptgroup("80 - Display")
		interest(1)
		prop(YES)
	}
	field(HIHI,DBF_DOUBLE) {
		prompt("Hihi Alarm Limit")
		promptgroup("70 - Alarm")
		pp(TRUE)
		interest(1)
		prop(YES)
	}
	field(LOLO,DBF_DOUBLE) {
		prompt("Lolo Alarm Limit")
		promptgroup("70 - Alarm")
		pp(TRUE)
		interest(1)
		prop(YES)
	}
	field(HIGH,DBF_DOUBLE) {
		prompt("High Alarm Limit")
		promptgroup("70 - Alarm")
		pp(TRUE)
		interest(1)
		prop(YES)
	}
	field(LOW,DBF_DOUBLE) {
		prompt("Low Alarm Limit")
		promptgroup("70 - Alarm")
		pp(TRUE)
		interest(1)
		prop(YES)
	}
	field(HHSV,DBF_MENU) {
		prompt("Hihi Severity")
		promptgroup("70 - Alarm")
		pp(TRUE)
		interest(1)
		prop(YES)
		menu(menuAlarmSevr)
	}
	field(LLSV,DBF_MENU) {
		prompt("Lolo Severity")
		promptgroup("70 - Alarm")
		pp(TRUE)
		interest(1)
		prop(YES)
		menu(menuAlarmSevr)
	}
	field(HSV,DBF_MENU) {
		prompt("High Severity")
		promptgroup("70 - Alarm")
		pp(TRUE)
		interest(1)
		prop(YES)
		menu(menuAlarmSevr)
	}
	field(LSV,DBF_MENU) {
		prompt("Low Severity")
		promptgroup("70 - Alarm")
		pp(TRUE)
		interest(1)
		prop(YES)
		menu(menuAlarmSevr)
	}
	field(HYST,DBF_DOUBLE) {
		prompt("Alarm Deadband")
		promptgroup("70 - Alarm")
		interest(1)
	}
	field(ADEL,DBF_DOUBLE) {
		prompt("Archive Deadband")
		promptgroup("80 - Display")
		interest(1)
	}
	field(MDEL,DBF_DOUBLE) {
		prompt("Monitor Deadband")
		promptgroup("80 - Display")
		interest(1)
	}
	field(A,DBF_DOUBLE) {
		prompt("Value of Input A")
		pp(TRUE)
	}
	field(B,DBF_DOUBLE) {
		prompt("Value of Input B")
		pp(TRUE)
	}
	field(C,DBF_DOUBLE) {
		prompt("Value of Input C")
		pp(TRUE)
	}
	field(D,DBF_DOUBLE) {
		prompt("Value of Input D")
		pp(TRUE)
	}
	field(E,DBF_DOUBLE) {
		prompt("Value of Input E")
		pp(TRUE)
	}
	field(F,DBF_DOUBLE) {
		prompt("Value of Input F")
		pp(TRUE)
	}
	field(G,DBF_DOUBLE) {
		prompt("Value of Input G")
		pp(TRUE)
	}
	field(H,DBF_DOUBLE) {
		prompt("Value of Input H")
		pp(TRUE)
	}
	field(I,DBF_DOUBLE) {
		prompt("Value of Input I")
		pp(TRUE)
	}
	field(J,DBF_DOUBLE) {
		prompt("Value of Input J")
		pp(TRUE)
	}
	field(K,DBF_DOUBLE) {
		prompt("Value of Input K")
		pp(TRUE)
	}
	field(L,DBF_DOUBLE) {
		prompt("Value of Input L")
		pp(TRUE)
	}
	field(LA,DBF_DOUBLE) {
		prompt("Prev Value of A")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LB,DBF_DOUBLE) {
		prompt("Prev Value of B")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LC,DBF_DOUBLE) {
		prompt("Prev Value of C")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LD,DBF_DOUBLE) {
		prompt("Prev Value of D")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LE,DBF_DOUBLE) {
		prompt("Prev Value of E")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LF,DBF_DOUBLE) {
		prompt("Prev Value of F")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LG,DBF_DOUBLE) {
		prompt("Prev Value of G")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LH,DBF_DOUBLE) {
		prompt("Prev Value of H")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LI,DBF_DOUBLE) {
		prompt("Prev Value of I")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LJ,DBF_DOUBLE) {
		prompt("Prev Value of J")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LK,DBF_DOUBLE) {
		prompt("Prev Value of K")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LL,DBF_DOUBLE) {
		prompt("Prev Value of L")
		special(SPC_NOMOD)
		interest(3)
	}
	field(LALM,DBF_DOUBLE) {
		prompt("Last Value Alarmed")
		special(SPC_NOMOD)
		interest(3)
	}
	field(ALST,DBF_DOUBLE) {
		prompt("Last Value Archived")
		special(SPC_NOMOD)
		interest(3)
	}
	field(MLST,DBF_DOUBLE) {
		prompt("Last Val Monitored")
		special(SPC_NOMOD)
		interest(3)
	}
	field(NLST,DBF_USHORT) {
		prompt("Last Index Monitored")
		special(SPC_NOMOD)
		interest(3)
	}
}
