    General
- Look at Marty's comments, respond
- Documentation
- Performance measurements
- Implement and improve connection management
- Make any asynBusy record, same as bo, except:
    - Does not call recGblFwdLink until VAL=0.
    - Soft device support is same as bo record.
    - Flag indicating callback from device support, don't write output.

    asynParamBase
- Make it handle array interfaces with pointers?

    NDPluginBase
- Add all 10 dimensions to database
  
    drvNDFile
- Test reading

    drvNDStdArrays

    drvNDROI
- Add cross-sections

    drvSimDetector driver
- Test all image data types with all waveform data types
- Add connection state

    drvProsilica driver
- Connection management
  - Sense disconnect, autoreconnect
  - Implement link callback.  When matches uniqueID, call Disconnect or Connect
- Support color
  
    Other drivers
- Roper using WinView/OLE
- Pilatus
- MAR-CCD
- MAR-345

   IDL
- Fix image_display
  - Make TVSCL image 
	Resizeable;
  - Change table widgets to text widgets or CW_field widgets
  - Use rotate rather than order keyword on tv
  - Check if data is byte and scaling is 0 to 255 don't scale the image
- Data saving?
