# This example if for running a motor record that uses the MX device
# driver support on a Unix host.  This example does not require Asyn.

# Start errlog Task before any possible error messsage to prevent
# erroneous "Interrupted system call" message on Linux OS host.
errlogInit(0)

dbLoadDatabase("../../dbd/NoAsyn.dbd",0,0)
registerRecordDeviceDriver(pdbbase) 
dbLoadRecords("../../db/NoAsyn_MX.db","user=rls")
MXmotorSetup(1, "MXexample.dat", 10)

iocInit()
