# RELEASE - Location of external products
#
# Note: This file will be scanned to automatically generate
#       include path definitions etc.
#       The order of the following declarations will be retained
#       within those definitions.
#
# Note that "#!" marks lines that can be uncommented.
#
# Add your declarations here

SUPPORT=/path/to/support

# If any motor controller communication mechanism besides 
# the VME backplane is required, then ASYN must be defined.
# Recommended ASYN release: R4-35
ASYN=$(SUPPORT)/asyn-R4-35

# Need the sequencer and the busy record for trajectory scanning
# Recommended SNCSEQ release: R2.2.6
SNCSEQ=$(SUPPORT)/seq-2-2-6
# Recommended BUSY release: R1-7-1
BUSY=$(SUPPORT)/busy-R1-7-1

# Recommended EPICS release: R3.15.6
EPICS_BASE=/path/to/base

# The following must be defined for motorMXmotor
#!MX=$(SUPPORT)/mx/mx

# IPAC is required to build motorHytec
# Recommended IPAC release: R2-15
IPAC=$(SUPPORT)/ipac-R2-15

# Script module needed to build motorScriptMotor
#!LUA=$(SUPPORT)/lua-R1-3

# Modbus module needed to build motorAMCI's example IOC
# Required MODBUS release: R2-11 or later
#!MODBUS=$(SUPPORT)/modbus-R2-11

# The following is only needed for the motor examples in iocBoot.
#!MOTOR=$(TOP)

# These lines allow developers to override these RELEASE settings
# without having to modify this file directly.
-include $(TOP)/../RELEASE.local
-include $(TOP)/../RELEASE.$(EPICS_HOST_ARCH).local
-include $(TOP)/configure/RELEASE.local
