! PGPLOT drivers.
!------------------------------------------------------------------------------
! To configure PGPLOT, ensure that drivers you do not want are
! commented out (place ! in column 1). N.B. Many device-drivers are
! available on selected operating systems only.
!------------------------------------------------------------------------------
! File       Code       Description                                Restrictions
! BCDRIV 0 /BCANON    Canon Laser printer (bitmap version), landscape
! CADRIV 0 /CANON     Canon Laser printer, LBP-8/A2, landscape
! CCDRIV 0 /CCP       DEC LJ250 Color Companion printer
! CGDRIV 1 /CGM       CGM metafile, indexed colour selection            C
! CGDRIV 2 /CGMD      CGM metafile, direct colour selection             C
! CWDRIV 0 /CW6320    Gould/Bryans Colourwriter 6320 pen plotter	Std F77
! EPDRIV 0 /EPSON     Epson FX100 dot matrix printer
! EXDRIV 1 /EXCL      Talaris/EXCL printers, landscape
! EXDRIV 2 /EXCL      Talaris/EXCL printers, portrait
! GCDRIV 0 /GENICOM   Genicom 4410 dot-matrix printer, landscape
!             Caution: use of GIDRIV may require a license from Unisys:
  GIDRIV 1 /GIF       GIF-format file, landscape
  GIDRIV 2 /VGIF      GIF-format file, portrait
! GLDRIV 1 /HPGL      Hewlett-Packard HP-GL plotters, landscape		Std F77
! GLDRIV 2 /VHPGL     Hewlett-Packard HP-GL plotters, portrait		Std F77
! GODRIV 0 /GOC       GOC Sigma T5670 terminal				VMS 
! GVDRIV 0 /GVENICOM  Genicom 4410 dot-matrix printer, portrait
! HGDRIV 0 /HPGL2     Hewlett-Packard graphics language
! HIDRIV 0 /HIDMP     Houston Instruments HIDMP pen plotter
! HJDRIV 0 /HJ        Hewlett-Packard Desk/Laserjet printer
! HPDRIV 0 /HP7221    Hewlett-Packard HP7221 pen plotter		Std F77
! LADRIV 0 /LA50      Dec LA50 and other sixel printers
! LJDRIV 0 /LJ        Hewlett-Packard LaserJet printers                 VMS
! LSDRIV 1 /LIPS2     Canon LaserShot printer (landscape)
! LSDRIV 2 /VLIPS2    Canon LaserShot printer (portrait)
! LNDRIV 0 /LN03      Dec LN03-PLUS Laser printer (landscape)           VMS
! LVDRIV 0 /LVN03     Dec LN03-PLUS Laser printer (portrait)            VMS
! LXDRIV 0 /LATEX     LaTeX picture environment
! MFDRIV 0 /FILE      PGPLOT graphics metafile
! NEDRIV 0 /NEXT      Computers running NeXTstep operating system
  NUDRIV 0 /NULL      Null device (no output)				Std F77
! PGDRIV 0 /PGMF      PGPLOT metafile (new format, experimental)        Std F77
! PNDRIV 1 /PNG       Portable Network Graphics file                    C
! PNDRIV 2 /TPNG      Portable Network Graphics file - transparent background C
! PPDRIV 1 /PPM       Portable Pixel Map file, landscape
! PPDRIV 2 /VPPM      Portable PIxel Map file, portrait
  PSDRIV 1 /PS        PostScript printers, monochrome, landscape	Std F77
  PSDRIV 2 /VPS       Postscript printers, monochrome, portrait		Std F77
  PSDRIV 3 /CPS       PostScript printers, color, landscape		Std F77
  PSDRIV 4 /VCPS      PostScript printers, color, portrait		Std F77
! PXDRIV 0 /PRINTRONI Printronix P300 or P600 dot-matrix printer
! QMDRIV 1 /QMS       QUIC devices (QMS and Talaris), landscape		Std F77
! QMDRIV 2 /VQMS      QUIC devices (QMS and Talaris), portrait		Std F77
! TFDRIV 0 /TFILE     Tektronix-format disk file                        VMS
! TODRIV 0 /TOSHIBA   Toshiba "3-in-one" printer, model P351
! TTDRIV 1 /TEK4010   Tektronix 4006/4010 storage-tube terminal		Std F77
! TTDRIV 2 /GF        GraphOn terminal					Std F77
! TTDRIV 3 /RETRO     RetroGraphics terminal				Std F77
! TTDRIV 4 /GTERM     GTERM Tektronix terminal emulator			Std F77
  TTDRIV 5 /XTERM     XTERM Tektronix terminal emulator			Std F77
! TTDRIV 6 /ZSTEM     ZSTEM terminal emulator				Std F77
! TTDRIV 7 /V603      Visual 603 terminal				Std F77
! TTDRIV 8 /KRM3      Kermit 3 on IBM-PC				Std F77
! TTDRIV 9 /TK4100    Tektronix 4100-series terminals			Std F77
! TTDRIV 10 /VMAC     Macintosh VersaTerm-PRO Tektronix-4105 emulator	Std F77
! TXDRIV 0 /TX        TeX PK Font Output files
! VADRIV 0 /VCANON    Canon Laser printer, LBP-8/A2, portrait
! VBDRIV 0 /VBCANON   Canon Laser printer (bitmap version), portrait
! VTDRIV 0 /VT125     Dec Regis terminals (VT125 etc.)			Std F77
! WDDRIV 1 /WD        X Window dump file, landscape
! WDDRIV 2 /VWD       X Window dump file, portrait
! WSDRIV 0 /WS        VAX workstations running VWS software		VMS
! X2DRIV 0 /XDISP     PGDISP or FIGDISP server for X workstations	C
  XWDRIV 1 /XWINDOW   Workstations running X Window System		C
  XWDRIV 2 /XSERVE    Persistent window on X Window System		C
! ZEDRIV 0 /ZETA      Zeta 8 Digital Plotter
!
! The following drivers can only be used in PGPLOT installations on MS-DOS
! systems with appropriate hardware and software. Do not select these 
! on UNIX or VMS systems.
!
! LHDRIV 0 /LH        IBM PCs and clones, Lahey F77 32-bit Fortran v5.0
! MSDRIV 0 /MSOFT     IBM PCs and clones running Microsoft Fortran 5.0
! SSDRIV 0 /SS        IBM PCs and clones, MS-DOS, Salford Software FTN
!
! The following driver can only be used in PGPLOT installations on Acorn
! Archimedes systems with appropriate hardware and software.
!
! ACDRIV 0 /ARC       Acorn Archimedes computer
!
! Selection of the XMOTIF driver causes a stub driver to be placed in
! the main PGPLOT library. The real driver is placed in libXmPgplot.a.
! Applications that need the Motif driver should link with libXmPgplot.a
! before the PGPLOT library. This treatment means that only Motif
! applications have to be linked with Motif libraries.
!
! XMDRIV 0 /XMOTIF    Motif applications containing XmPgplot widgets.   C
!
! Selection of the XATHENA driver causes a stub driver to be placed in
! the main PGPLOT library. The real driver is placed in libXawPgplot.a.
! Applications that need the Athena driver should link with libXawPgplot.a
! before the PGPLOT library. This treatment means that only Athena
! applications have to be linked with Xaw libraries.
!
! XADRIV 0 /XATHENA    Motif applications containing XaPgplot widgets.   C
!
! Selection of the TK driver causes a stub driver to be placed in
! the main PGPLOT library. The real driver is placed in libtkpgplot.a.
! Applications that need the Tk driver should link with libtkpgplot.a
! before the PGPLOT library. This treatment means that only Tcl/Tk
! applications have to be linked with the Tcl and Tk libraries.
!
! TKDRIV 0 /XTK       X-window Tcl/Tk programs with pgplot widgets.     C
!
! The following driver is included solely for use by the aips++ team.
!
! RVDRIV 0 /XRV       X-window Rivet/Tk programs with pgplot widgets.   C
