[NODE]
description = PGAS5 gas pressure cell stick 
id = pgas5.stick.sea.psi.ch

[sea_stick]
class = secop_psi.sea.SeaClient
description = stick SEA connection to ill5.stick
config = ill5.stick
service = stick

[ts]
class = secop_psi.sea.SeaReadable
io = sea_stick
sea_object = tt
json_file = ill5.config.json
rel_paths = ts

[T_bottom]
class = secop_psi.sea.SeaReadable
io = sea_stick
sea_object = tt
json_file = ill5.config.json
rel_paths = tb
