stickDesc = oven stick for SANS 

makenv ts -driver 336_lsc -controller _tt {
  lsc_sensor ts C -sensor pt1000e -sensorname sample -color blue
  lsc_sensor ts_2 D -sensor pt1000e -sensorname sample2 -color orange
  lsc_loop set -loop 2 -channel C -maxheater 62.5W -resist 40Ohm -loopname sample -color dark_green
} {C D}

catch {
ts ts/alarm 675
ts setsamp/limit 670
ts setsamp/ramp 20
ts setsamp/resist 50
ts setsamp/maxheater 50W
}
