stickDesc = 50 mm calibration stick (ORI1/ORI2/ILL1), version with standard lsc370 driver

makenv res -driver 370_lsc {
  lsc_sensor s1 -channel 1 -sensor raw -excitation 200uV
  lsc_sensor s2 -channel 2 -sensor raw -excitation 200uV
  lsc_sensor s3 -channel 3 -sensor X75610 -excitation 200uV
  lsc_sensor s4 -channel 4 -sensor raw -excitation 200uV
  lsc_sensor s5 -channel 5 -sensor raw -excitation 200uV
  lsc_sensor s6 -channel 6 -sensor raw -excitation 200uV
}

GraphAdd res.s1.raw Ohm R1
GraphAdd res.s2.raw Ohm R2
GraphAdd res.s3.raw Ohm R3
GraphAdd res.s4.raw Ohm R4
GraphAdd res.s5.raw Ohm R5
GraphAdd res.s6.raw Ohm R6

res autoscan/interval 15
res autoscan/pause 5
res autoscan/dwell 5

makenv calib -driver zcalib

# first and last points with smaller step
# steps are about 3%, 6%, 10% (57x), 5%, 2.5%
# with ORI2, nv set 1.1 the base T is ~ 1.37 K

calib tlist 1.38 1.42 1.51 logstep0.04 288 302 310

# timing is such that 2 * 24h are not enough
# try with a little more precision (expecially at hi T)

calib slopelimit 0.005
