stickDesc = stick 1 MuSR flow

makenv ts -driver [lsdriver _ts] {
# lsc_sensor ts A -sensor x75239 -sensorname sample
 lsc_sensor tc B -sensor x85569 -sensorname sample
# lsc_loop set -loop 1 -channel A -maxheater 50W -resist 50Ohm
}

