stickDesc = high voltage stick (short can)

makenv hcp hcp
appendVars hcp/V/Voltage hcp.workset/V/Set hcp.current/A/Current
stick_sensors x50923 undefined


#makenv fn -driver fungen -port localhost:3015


#kthMake ldmcc03-ts:3004
#appendVars kth/pA/Kth/1 kth.volt/V/Volt/2
#kth file /home/sans/kth
#kth time0 2
#kth time 10


# make ts_2 the "sample" sensor
#hsetprop /tt getsample "hval /tt/ts_2"
makenv HV -driver drvpar /hcp

GraphAdd hcp V Voltage green
GraphAdd hcp.current A current red
GraphAdd hcp.workset V V_set dark_green

# create drivable for TASMAD
makenv i1 -driver drvpar /hcp
