addonDesc = ultrasound with SP devices data acquisition card and function generator

set ::secop_version 4

makenv ultrasound -driver secop
#makenv ultrasound -driver secop ALL restart_on_reconnect


GraphAdd roi0.i 1 inphase

GraphAdd f.slope 2 slope
GraphAdd f Hz freq

makenv fn -driver fungen -port A-33210A-12987.psi.ch:5025

catch {
  fn burst 0
  fn waveform PULS
  fn offset 0.675
  fn volt 1.35
  fn freq 1000
  fn width 200e-9
}

makenv mirror -driver mirror pars

