# CCU4 configuration table
# All items must be TAB separated
#
# Device: max length 6
# Ra/Rb: coding resistor values [kOhm]
# Options:
#   f: nv flow
#   n: LN2 sensor with autofill 
#   N: LN2 autofill with external level meter
#   a: LHe level sensor compatible with AMI (HeCurr 75, HeWiRes 460)
#   o: LHe level sensor compatible with Oxford ILM (HeCurr 130, HeWiRes 166)
#   h: other LHe level sensor (HeCurr and HeWiRes must be given)
#   H: LHe autofill with external level meter
# HeLen total length of He level sensor [mm]
# HeTop unused length of He level sensor at the top [mm]
# HeCurr LHe sensor energization current [mA]
# HeWiRes LHe sensor wire resitivity [Ohm/m]
#
#
#Device	Ra	Rb	Options	HeLen	HeTop	HeCurr	HeWiRes
#--------------------------------------------------------------
none				
ILL1	0.22		fna	380	26
ILL2	0.33		fna	380	26
ILL3	0.47		fna	380	7
ILL4	47		fna	380	0
ILL5	0.82		fna	520	24
VARIOX	1		fno	355	8
ORI1	1.2		fno	400	74
ORI2	1.5		fno	400	74
ORI3	1.8		fno	450	4
ORI4	2.2		fna	520	24
ORI6	0.1		fna	520	24
MA02	4.7		fnH	
MA09	5.6		fH	
MA11	6.8		fNH	
MA15	8.2		fNH	
MA6	12		fNH	
MA7	15		fNH	
MA10	22		fNH
MB11			NH
#CTI1		0.22		
CTI2		0.33		
CTI4		0.68		
CTI5		0.82		
#CTI7		1		
DISC		1.2		
DISE		1.5		
APD		1.8		
CCR2HT		2.7		
CCR3		3.3		
CCR4		0.47		
CCRPE		3.9	f
RSE		12		
RT		15
JTVALV	10		n
JTCCR	18		n
LOLLYP			fa	550	200
HE3ANN			h	38	105	95	460
MANGO			fh	550	200	95	88
HEOX		0.1	fo	459	250
FFTF			fNH
MB11			NH
HALFLOW			f
LEMFLOW			f
