stickDesc = high voltage stick (extended can)

makenv hcp hcp
appendVars hcp/V/Voltage hcp.workset/V/Set hcp.current/A/Current

stick_sensors x50923 x63854


#makenv fn -driver fungen -port localhost:3015


#kthMake ldmcc03-ts:3004
#appendVars kth/pA/Kth/1 kth.volt/V/Volt/2
#kth file /home/sans/kth
#kth time0 2
#kth time 10


# make ts_2 the "sample" sensor
#hsetprop /tt getsample "hval /tt/ts_2"


