**Hey, look at my nice data!**  
What a load of bs!  
**Oy, no need to be rude!**  
I'm not!  I mean, what a load of beam synchronous data!  
**Well, thanks, but it is not all saved**
Bummer, how were you saving it?  
**I used this cool command line script bs...**  
I'm going to stop you there  
**But my BS command works; there must be a problem with the sources!**  
Try each one individually with the bs command..  
**OK, hang on, what the!  They work, the both save individually!**  
Yes the issue is when you try and save sources from different IOCs/devices with the bs command 
