\chapter{aare}
\hypertarget{index}{}\label{index}\index{aare@{aare}}
\label{index_md_README}%
\Hypertarget{index_md_README}%
Data analysis library for PSI hybrid detectors\hypertarget{index_autotoc_md1}{}\doxysection{\texorpdfstring{Folder structure}{Folder structure}}\label{index_autotoc_md1}
\tabulinesep=1mm
\begin{longtabu}spread 0pt [c]{*{3}{|X[-1]}|}
\hline
\PBS\centering \cellcolor{\tableheadbgcolor}\textbf{ Folder   }&\PBS\centering \cellcolor{\tableheadbgcolor}\textbf{ subfolder   }&\PBS\centering \cellcolor{\tableheadbgcolor}\textbf{ Content    }\\\cline{1-3}
\endfirsthead
\hline
\endfoot
\hline
\PBS\centering \cellcolor{\tableheadbgcolor}\textbf{ Folder   }&\PBS\centering \cellcolor{\tableheadbgcolor}\textbf{ subfolder   }&\PBS\centering \cellcolor{\tableheadbgcolor}\textbf{ Content    }\\\cline{1-3}
\endhead
include/   &aare/   &top level header/s    \\\cline{1-3}
core/   &include/   &public headers for core    \\\cline{1-3}
&src/   &source files and non public headers   \\\cline{1-3}
\end{longtabu}
\hypertarget{index_autotoc_md2}{}\doxysection{\texorpdfstring{file\+\_\+io class diagram}{file\_io class diagram}}\label{index_autotoc_md2}
\hypertarget{index_autotoc_md3}{}\doxysection{\texorpdfstring{Test the zmq socket with a detector simulator}{Test the zmq socket with a detector simulator}}\label{index_autotoc_md3}
{\bfseries{1. Download and build the sls\+Detector\+Package}}


\begin{DoxyCode}{0}
\DoxyCodeLine{git\ clone\ https://github.com/slsdetectorgroup/slsDetectorPackage.git\ -\/-\/branch=8.0.1\ \#or\ the\ desired\ branch}
\DoxyCodeLine{cd\ slsDetectorPackage}
\DoxyCodeLine{mkdir\ build\ \&\&\ cd\ build}
\DoxyCodeLine{cmake\ ..\ -\/DSLS\_USE\_SIMULATOR=ON}
\DoxyCodeLine{make\ -\/j8\ \#or\ your\ number\ of\ cores}

\end{DoxyCode}


{\bfseries{2. Launch the sls\+Receiver}} 
\begin{DoxyCode}{0}
\DoxyCodeLine{bin/slsReceiver}

\end{DoxyCode}


{\bfseries{3. Launch the virtual server}} 
\begin{DoxyCode}{0}
\DoxyCodeLine{bin/jungfrauDetectorServer\_virtual}

\end{DoxyCode}


{\bfseries{4 Configure the detector simulator}}


\begin{DoxyCode}{0}
\DoxyCodeLine{\#sample\ config\ file\ is\ in\ etc/\ in\ the\ aare\ repo}
\DoxyCodeLine{sls\_detector\_put\ config\ etc/virtual\_jf.config}
\DoxyCodeLine{}
\DoxyCodeLine{\#Now\ you\ can\ take\ images\ using\ sls\_detector\_acquire}
\DoxyCodeLine{sls\_detector\_acquire}

\end{DoxyCode}


{\bfseries{5. Run the zmq example}} 
\begin{DoxyCode}{0}
\DoxyCodeLine{examples/zmq\_example}
\DoxyCodeLine{}
\DoxyCodeLine{\#Will\ print\ the\ headers\ fof\ the\ frames\ received}

\end{DoxyCode}
\hypertarget{index_autotoc_md4}{}\doxysection{\texorpdfstring{Test the zmq processing replaying data}{Test the zmq processing replaying data}}\label{index_autotoc_md4}
To be implemented\hypertarget{index_autotoc_md5}{}\doxysection{\texorpdfstring{generate documentation}{generate documentation}}\label{index_autotoc_md5}

\begin{DoxyCode}{0}

\end{DoxyCode}
 