\section{angle\-Conversion\-Constant Struct Reference}
\label{structangleConversionConstant}\index{angleConversionConstant@{angleConversionConstant}}
{\tt \#include $<$sls\_\-detector\_\-defs.h$>$}

\subsection*{Public Attributes}
\begin{CompactItemize}
\item 
float \bf{center}
\item 
float \bf{ecenter}
\item 
float \bf{r\_\-conversion}
\item 
float \bf{er\_\-conversion}
\item 
float \bf{offset}
\item 
float \bf{eoffset}
\item 
float \bf{tilt}
\item 
float \bf{etilt}
\end{CompactItemize}


\subsection{Detailed Description}
angular conversion constant for a module 



\subsection{Member Data Documentation}
\index{angleConversionConstant@{angle\-Conversion\-Constant}!center@{center}}
\index{center@{center}!angleConversionConstant@{angle\-Conversion\-Constant}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}float \bf{angle\-Conversion\-Constant::center}}\label{structangleConversionConstant_3e4a757b4b527bdc68872d62e071dffc}


center of the module (channel at which the radius is perpendicular to the module surface) \index{angleConversionConstant@{angle\-Conversion\-Constant}!ecenter@{ecenter}}
\index{ecenter@{ecenter}!angleConversionConstant@{angle\-Conversion\-Constant}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}float \bf{angle\-Conversion\-Constant::ecenter}}\label{structangleConversionConstant_9927754f8e0f20a6315b423e265a7431}


error in the center determination \index{angleConversionConstant@{angle\-Conversion\-Constant}!eoffset@{eoffset}}
\index{eoffset@{eoffset}!angleConversionConstant@{angle\-Conversion\-Constant}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}float \bf{angle\-Conversion\-Constant::eoffset}}\label{structangleConversionConstant_f49909ae584f5c00fd7417a0a7cfb28c}


error in the offset determination \index{angleConversionConstant@{angle\-Conversion\-Constant}!er_conversion@{er\_\-conversion}}
\index{er_conversion@{er\_\-conversion}!angleConversionConstant@{angle\-Conversion\-Constant}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}float \bf{angle\-Conversion\-Constant::er\_\-conversion}}\label{structangleConversionConstant_123c4b9d22c2bc6c8a00eac0a31faeb3}


error in the r\_\-conversion determination \index{angleConversionConstant@{angle\-Conversion\-Constant}!etilt@{etilt}}
\index{etilt@{etilt}!angleConversionConstant@{angle\-Conversion\-Constant}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}float \bf{angle\-Conversion\-Constant::etilt}}\label{structangleConversionConstant_6b7c4f3e7ac444fefd3b3957b25fa27f}


error in the tilt determination \index{angleConversionConstant@{angle\-Conversion\-Constant}!offset@{offset}}
\index{offset@{offset}!angleConversionConstant@{angle\-Conversion\-Constant}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}float \bf{angle\-Conversion\-Constant::offset}}\label{structangleConversionConstant_2d71e0c6f0eb37f96743961f1d051e5f}


the module offset i.e. the position of channel 0 with respect to the diffractometer 0 \index{angleConversionConstant@{angle\-Conversion\-Constant}!r_conversion@{r\_\-conversion}}
\index{r_conversion@{r\_\-conversion}!angleConversionConstant@{angle\-Conversion\-Constant}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}float \bf{angle\-Conversion\-Constant::r\_\-conversion}}\label{structangleConversionConstant_30dec69c8f1e62c582ad18f67f293bf3}


detector pixel size (or strip pitch) divided by the diffractometer radius \index{angleConversionConstant@{angle\-Conversion\-Constant}!tilt@{tilt}}
\index{tilt@{tilt}!angleConversionConstant@{angle\-Conversion\-Constant}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}float \bf{angle\-Conversion\-Constant::tilt}}\label{structangleConversionConstant_23af3f7c89696b83abb6a713061cc4b9}


ossible tilt in the orthogonal direction (unused) 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
common\-Files/\bf{sls\_\-detector\_\-defs.h}\end{CompactItemize}
