#*************************************************************************
# Copyright (c) 2002 The University of Chicago, as Operator of Argonne
#     National Laboratory.
# Copyright (c) 2002 The Regents of the University of California, as
#     Operator of Los Alamos National Laboratory.
# EPICS BASE Versions 3.13.7
# and higher are distributed subject to a Software License Agreement found
# in file LICENSE that is included with this distribution. 
#*************************************************************************
menu(compressALG) {
	choice(compressALG_N_to_1_Low_Value,"N to 1 Low Value")
	choice(compressALG_N_to_1_High_Value,"N to 1 High Value")
	choice(compressALG_N_to_1_Average,"N to 1 Average")
	choice(compressALG_Average,"Average")
	choice(compressALG_Circular_Buffer,"Circular Buffer")
	choice(compressALG_N_to_1_Median,"N to 1 Median")
}
recordtype(compress) {
	include "dbCommon.dbd" 
	field(VAL,DBF_NOACCESS) {
		prompt("Value")
		asl(ASL0)
		special(SPC_DBADDR)
		pp(TRUE)
		extra("void *		val")
	}
	field(INP,DBF_INLINK) {
		prompt("Input Specification")
		promptgroup(GUI_COMPRESS)
		interest(1)
	}
	field(RES,DBF_SHORT) {
		prompt("Reset")
		asl(ASL0)
		special(SPC_RESET)
		interest(3)
	}
	field(ALG,DBF_MENU) {
		prompt("Compression Algorithm")
		promptgroup(GUI_ALARMS)
		special(SPC_RESET)
		interest(1)
		menu(compressALG)
	}
	field(NSAM,DBF_ULONG) {
		prompt("Number of Values")
		promptgroup(GUI_COMPRESS)
		special(SPC_NOMOD)
		interest(1)
		initial("1")
	}
	field(N,DBF_ULONG) {
		prompt("N to 1 Compression")
		promptgroup(GUI_COMPRESS)
		special(SPC_RESET)
		interest(1)
		initial("1")
	}
	field(IHIL,DBF_DOUBLE) {
		prompt("Init High Interest Lim")
		promptgroup(GUI_COMPRESS)
		interest(1)
	}
	field(ILIL,DBF_DOUBLE) {
		prompt("Init Low Interest Lim")
		promptgroup(GUI_COMPRESS)
		interest(1)
	}
	field(HOPR,DBF_DOUBLE) {
		prompt("High Operating Range")
		promptgroup(GUI_DISPLAY)
		interest(1)
	}
	field(LOPR,DBF_DOUBLE) {
		prompt("Low Operating Range")
		promptgroup(GUI_DISPLAY)
		interest(1)
	}
	field(PREC,DBF_SHORT) {
		prompt("Display Precision")
		promptgroup(GUI_DISPLAY)
		interest(1)
	}
	field(EGU,DBF_STRING) {
		prompt("EngineeringUnits")
		promptgroup(GUI_DISPLAY)
		interest(1)
		size(16)
	}
	field(OFF,DBF_ULONG) {
		prompt("Offset")
		special(SPC_NOMOD)
	}
	field(NUSE,DBF_ULONG) {
		prompt("Number Used")
		special(SPC_NOMOD)
	}
	field(BPTR,DBF_NOACCESS) {
		prompt("Buffer Pointer")
		special(SPC_NOMOD)
		interest(4)
		extra("double		*bptr")
	}
	field(SPTR,DBF_NOACCESS) {
		prompt("Summing Buffer Ptr")
		special(SPC_NOMOD)
		interest(4)
		extra("double		*sptr")
	}
	field(WPTR,DBF_NOACCESS) {
		prompt("Working Buffer Ptr")
		special(SPC_NOMOD)
		interest(4)
		extra("double		*wptr")
	}
	field(INPN,DBF_LONG) {
		prompt("Number of elements in Working Buffer")
		special(SPC_NOMOD)
		interest(4)
	}
	field(CVB,DBF_DOUBLE) {
		prompt("Compress Value Buffer")
		special(SPC_NOMOD)
		interest(3)
	}
	field(INX,DBF_ULONG) {
		prompt("Compressed Array Inx")
		special(SPC_NOMOD)
		interest(3)
	}
}
