# CONFIG_SITE.linux-x86.Common
#
# Site override definitions for linux-x86 host builds
#-------------------------------------------------------

#CROSS_COMPILER_TARGET_ARCHS = vxWorks-ppc32
#CROSS_COMPILER_TARGET_ARCHS = RTEMS-mvme2100 RTEMS-pc386-qemu

INSTALL_LOCATION=/usr/local/epics/base-$(EPICS_VERSION).$(EPICS_REVISION).$(EPICS_MODIFICATION)

GNU_HOST_ARCH=i686
GNU_HOST_OS=linux

# LD_LIBRARY_PATH may cause problems for eldk53-ppc4xxFP
LD_LIBRARY_PATH=

# vxWorks 5.5 for MVxxxx boards
CROSS_COMPILER_TARGET_ARCHS += T2-ppc604

# vxWorks 6.7 for MVxxxx boards
#CROSS_COMPILER_TARGET_ARCHS += V67-ppc604

# vxWorks 6.9 for MVxxxx boards
CROSS_COMPILER_TARGET_ARCHS += V69-ppc604
#CROSS_COMPILER_TARGET_ARCHS += V69-ppc32

# NI compact RIO
CROSS_COMPILER_TARGET_ARCHS += V63-ppc603

# MOXA montavista linux (No PVA because of missing boost support)
CROSS_COMPILER_TARGET_ARCHS += mvl40-xscale_be

# MOXA SDK 4.2
CROSS_COMPILER_TARGET_ARCHS += moxa42-armv6l

# Virtex embedded PPC
CROSS_COMPILER_TARGET_ARCHS += eldk51-ppc4xxSF

# IOxOS IFC1210
CROSS_COMPILER_TARGET_ARCHS += eldk52-e500v2

# DeltaTau PowerPMAC
CROSS_COMPILER_TARGET_ARCHS += eldk42-ppc4xxFP
CROSS_COMPILER_TARGET_ARCHS += eldk53-ppc4xxFP

# Test other vxWorks versions
#CROSS_COMPILER_TARGET_ARCHS += V66-ppc603
#CROSS_COMPILER_TARGET_ARCHS += V66-ppc604
#CROSS_COMPILER_TARGET_ARCHS += V63-ppc604
#CROSS_COMPILER_TARGET_ARCHS += V64-ppc604
# (No PVA because of old compiler)
#CROSS_COMPILER_TARGET_ARCHS += V62-ppc604

# Raspberry Pi
CROSS_COMPILER_TARGET_ARCHS += raspbian-arm

# RTEMS (Can only have 1 RTEMS major version in 1 EPICS installation
# because they overwrite their header files.)
#CROSS_COMPILER_TARGET_ARCHS += RTEMS49-pc386
CROSS_COMPILER_TARGET_ARCHS += RTEMS51-pc686
