#- Example vxWorks startup file

#- The following is needed if your board support package doesn't at boot time
#- automatically cd to the directory containing its startup script
#cd "_TOP_/iocBoot/_IOC_"

< cdCommands
#< ../nfsCommands

cd topbin

#- You may have to change _APPNAME_ to something else
#- everywhere it appears in this file
ld 0,0, "_APPNAME_.munch"

## Register all support components
cd top
dbLoadDatabase "dbd/_APPNAME_.dbd"
_CSAFEAPPNAME__registerRecordDeviceDriver pdbbase

## Load record instances
dbLoadTemplate "db/user.substitutions"
dbLoadRecords "db/_APPNAME_Version.db", "user=_USER_"
dbLoadRecords "db/dbSubExample.db", "user=_USER_"

#- Set this to see messages from mySub
#mySubDebug = 1

#- Run this to trace the stages of iocInit
#traceIocInit

cd startup
iocInit

## Start any sequence programs
#seq &sncExample, "user=_USER_"
