# RELEASE - Location of external products
#
# Note: This file will be scanned to automatically generate
#       include path definitions etc.
#       The order of the following declarations will be retained
#       within those definitions.
#
# Note that "#!" marks lines that can be uncommented.
#
# Add your declarations here

#!GATEWAY=
#!SUPPORT=

# If any motor controller communication mechanism besides the VME backplane is
# required, then ASYN must be defined.
# Recommended ASYN release: R4-10
ASYN=$(SUPPORT)/asyn/4-10

# Need the sequencer for the MM4005 and XPS trajectory scanning
# Recommended SNCSEQ release: R2-0-12
SNCSEQ=$(SUPPORT)/seq/2-0-12

# Recommended EPICS release: R3.14.10
EPICS_BASE=$(SUPPORT)/../base-3.14.10

# The following must be defined for the MXmotor device driver.
#!MX=$(SUPPORT)/mx/mx

# The following support modules are required ONLY if the examples in
# <motor>/motorExApp are built.  To build examples, the top Makefile,
# <motor>/Makefile must also be edited.

# Recommended IPAC release: R2-10
#!IPAC=$(SUPPORT)/ipacR2-10

# The following is only needed for the motor examples in iocBoot.
#!MOTOR=$(TOP)

