
/*--------------------------------------------------------------------------
                       A m o r 2 T . i
  Internal data structure definitions for Amor2T. For details see amor2t.tex.
  DO NOT TOUCH! This file is automatically created from amor2t.w.

  Mark Koennecke, September 1999
----------------------------------------------------------------------------*/

/* distance detector sample */
#define PARDS  0
/* constant height of sample: height = PARDH + MOTSOZ + MOTSTZ */
#define PARDH  1
/* distance diaphragm 4 - sample */
#define PARDD4 2
/* distance to diaphragm 5 */
#define PARDD5 3
/* interrupt to issue when a motor fails on this */
#define PARINT 4
/* base height of counter station */
#define PARDDH 5
/* height of D4 */
#define PARD4H 6
/* height of D5 */
#define PARD5H 7
/* base height of analyzer */
#define PARANA 8
/* distance of analyzer from sample */
#define PARADIS 9
/* flag analyzer calculation on/off */
#define ANAFLAG 10
/* constant for second detector */
#define PARDDD 11
/* constant part of AOM */
#define PARAOM 12


   typedef struct {
                    pMotor pMot;
                    char pName[80];
                    float fTarget;
                  }MotEntry, *pMotEntry;



  typedef struct __AMOR2T {
                            pObjectDescriptor pDes;
                            pIDrivable        pDriv;
                            pMotor            aEngine[MAXMOT];
                            MotEntry          toStart[MAXMOT];
                            int               iStart;
                            ObPar             *aParameter;
                          }Amor2T;


